 **GREYSTONE DATA TECHNOLOGY**

**40500A ALBRAE ST, FREMONT CA 94538**

|  |  |  |  |
| --- | --- | --- | --- |
| No. | Mfg. | Model | Status |
| 1 | BlackBerry | Q10 | Good |
| 2 | BlackBerry | Q10 | Good |
| 3 | BlackBerry | Z10 | BB Locked |
| 4 | BlackBerry | Z10 | Good |
| 5 | BlackBerry | Z30 | Good |
| 6 | BlackBerry | Z30 | Good |

\*If BlackBerry device is still locked, our current software does not support the latest update.

**Instructions**

1. Activate and complete phone set-up.

2. Tap Settings > Storage and Access.

3. Select USB connection > Connect to Windows (If the selected device has the option).

4. Select Access using Wi-Fi (Enter passcode - passwd).

5. Connect the device in a slot.

6. A window will appear to set the IP on the device.

7. Go to Security and Privacy > Device Password > Turn off Simple Password mode.

8. Tap Security and Privacy > Development mode.

9. Select Use Development Mode to ON. (Enter passcode – passwd)

10. Then set IP Address that is designated for that slot.

11. Tap ‘OK’ when a confirmation window appears.